DIREKTUR JENDERAL PERHUBUNGAN DARAT dengan ini menetapkan bahwa kendaraan bermotor :

(*Director General of Land Transport here by certifies the following vehicle*) :

|  |  |  |
| --- | --- | --- |
| MEREK*(Brand)* | : | ${brand} |
| TIPE *(Type)* | : | ${type} |
| JENIS *(Class)* | : | ${vehicle\_type} |
| PERUNTUKAN *(Purpose of Vehicle)* | : | ${purpose\_vehicle} |
| KENDARAAN YANG DIUJI *(the vehicle being tested)*   * NOMOR RANGKA (*Chassis Number* / VIN) * NOMOR MOTOR LISTRIK (*Electric Motor Number*) | :  : | ${chassis}  ${electric\_motor\_number} |
| TAHUN PEMBUATAN, PERAKITAN,KONVERSI  *(Year Of Manufacture, Assembly, Conversion)* | : | ${year\_build} |
| NAMA BENGKEL *(Workshop’s Name)* | : | ${workshop} |
| ALAMAT BENGKEL *(Workshop’s Address)* | : | ${address} |
| PENANGGUNG JAWAB *(Person in Charge)* | : | ${responsible\_person} |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| SPESIFIKASI TEKNIK KENDARAAN BERMOTOR / VARIAN (*Technilcal Spesification Of Motor Vehicle / Variant*) | | | | | |
| Konfigurasi  Sumbu  (*Axle Configuration*) | Jarak  Sumbu  (*Axle Distance*  */ Wheel Base*)  I – II  II – III  III – IV | Dimensi  (*Dimension*)  1. Lebar Total  (*Overall Width*)  2. Panjang Total  (*Overal*  *l Length*)  3. Tinggi Total  (*Overall Height*)  4. Julur Depan  (*Front Overhang*)  5. Julur Belakang  (*Rear Overhang*) | Daya Motor  Penggerak  Maksimum  (*Engine Power*) | Kapasitas Baterai  ( *Battery Capacity*) | Ukuran Ban  (*Tyre Size*)  1. Sumbu I  (*Ist axle*)  2. Sumbu II  (*2nd axle*)  3. Sumbu III  (*3rd axle*)  4. Sumbu IV  (*4th axle*) |
|  | ${axis\_1\_2} | ${width\_total} | ${power\_max} | ${battery\_max} | ${tire\_axis\_1} |
|  | ${axis\_2\_3} | ${length\_total} | ${tire\_axis\_2} |
|  | ${axis\_3\_4} | ${height\_total} | ${tire\_axis\_3} |
|  |  | ${julur\_front} | ${tire\_axis\_4} |
|  |  | ${julur\_rear} |  |  |  |

JBB / JBKB (*GVW/GCW*) : ${jbb}

BERAT KOSONG (*Curb Weight*) : ${empty\_weight}

JBI / JBKI (*GPVW/GPCW*) : ${jbi}

DAYA ANGKUT : ${carry\_capacity}, BARANG : ${goods\_capacity}

(*Pay Load*) (*Passanger Capacity including driver, luggage*)

KELAS JALAN TERENDAH YANG BOLEH DlLAUI (*Lowest road class permitted*): ${road\_class}

TEMPAT / TANGGAL UJI (*Place / Date ofTest*) : BPLJSKB, ${place\_test\_bpljskb} TANGGAL ${date\_bpljskb}

DINYATAKAN LULUS UJI TIPE KONVERSI SERTA MEMENUHI PERSYARATAN TEKNIS DAN LAIK JALAN.

(*Declared passed the type fest and fulfilling technical requirements and road worthiness*)

Jakarta, ${date}

Plt. DIREKTUR JENDERAL PERHUBUNGAN DARAT

(*Director General of Land Transportation*)

AHMAD YANI, A.T.D., M.T.

NIP. 19650930 199003 1 003